AS4111 RT Validation Test Report - Generated by AltaRTVal version 2.0.3.1
Date/Time: Monday, June 09, 2008, 7:58:19 AM

NOTE:  AltaRTVal ONLY performs the RT validation protocol (5.2) tests.
             Electrical (5.1) and Noise Rejection (5.3) tests are not part of this test.

SN:  Test Unit 12345 – Rev 1.2.4 – Company XYZ 

UUT Remote Terminal Information:
     RT Address = 0
     Supports Broadcast = True;  Supports Illegal Command = True;  Supports Variable Address = True
     Minimum number of data words = 1;  Maximum number of data words = 32
     Protocol:  MIL-STD-1553B Notice 2
     Redundancy:  DUAL (Bus A and Bus B)

Test Results:
  5.2 Protocol Tests - FAILED (Bus A - FAILED, Bus B - FAILED)
    5.2.1 Required Remote Terminal Operation - FAILED (Bus A - FAILED, Bus B - FAILED)
      5.2.1.1 Response to Command Words - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.1.1.1 RT Response to Command Words - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.1.1.2 RT to RT Response to Command Words - PASSED (Bus A - PASSED, Bus B - PASSED)

      5.2.1.2 Intermessage Gap - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.1.2.1 Minimum Time - PASSED (Bus A - PASSED, Bus B - PASSED)
              The minimum intermessage gap time during this test was 5.8us
              The maximum intermessage gap time during this test was 12.1us
        5.2.1.2.2 Transmission Rate - PASSED (Bus A - PASSED, Bus B - PASSED)
              The minimum intermessage gap time during this test was 5.8us
              The maximum intermessage gap time during this test was 8.6us

      5.2.1.3 Error Injection - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.1.3.1 Parity - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.1.1 Transmit Command Word - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.1.2 Receive Command Word - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.1.3 Receive Data Words - PASSED (Bus A - PASSED, Bus B - PASSED)

        5.2.1.3.2 Word Length - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.2.1 Transmit Command Word - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.2.2 Receive Command Word - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.2.3 Receive Data Words - PASSED (Bus A - PASSED, Bus B - PASSED)

        5.2.1.3.3 Bi-Phase Encoding - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.3.1 Transmit Command Word - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.3.2 Receive Command Word - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.3.3 Receive Data Words - PASSED (Bus A - PASSED, Bus B - PASSED)

        5.2.1.3.4 Sync Encoding - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.4.1 Transmit Command Word - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.4.2 Receive Command Word - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.4.3 Data Word - PASSED (Bus A - PASSED, Bus B - PASSED)

        5.2.1.3.5 Message Length - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.5.1 Transmit Command - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.5.2 Receive Command - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.5.3 Mode Command Word Count Error - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.1.3.5.4 RT to RT Word Count Error - PASSED (Bus A - PASSED, Bus B - PASSED)

        5.2.1.3.6 Contiguous Data - PASSED (Bus A - PASSED, Bus B - PASSED)

        5.2.1.3.7 Terminal Fail-Safe - Not Tested (Bus A - Not Tested, Bus B - Not Tested)

      5.2.1.4 Superseding Commands - Not Tested (Bus A - Not Tested, Bus B - Not Tested)
        5.2.1.4.1 RT Superseding Commands - Not Tested (Bus A - Not Tested, Bus B - Not Tested)
        5.2.1.4.2 RT to RT Superseding Commands - Not Tested (Bus A - Not Tested, Bus B - Not Tested)

      5.2.1.5 Required Mode Commands - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.1.5.1 Transmit Status - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.1.5.2 Transmitter Shutdown and Override - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.1.5.3 Reset Remote Terminal - PASSED (Bus A - PASSED, Bus B - PASSED)
           Bus A Reset Time = 4 microseconds
           Bus B Reset Time = 4 microseconds

      5.2.1.6 Data Wrap-Around - PASSED (Bus A - PASSED, Bus B - PASSED)

      5.2.1.7 RT to RT Message Errors - FAILED (Bus A - FAILED, Bus B - FAILED)
        5.2.1.7.1 RT to RT Timeout - FAILED (Bus A - FAILED, Bus B - FAILED)
        5.2.1.7.2 RT to RT Message Format Errors - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.1.7.3 Transmitting RT Errors - PASSED (Bus A - PASSED, Bus B - PASSED)

      5.2.1.8 Bus Switching - Not Tested (Bus A - Not Tested, Bus B - Not Tested)

      5.2.1.9 Unique Address - Not Tested (Bus A - Not Tested, Bus B - Not Tested)

    5.2.2 Optional Operation - PASSED (Bus A - PASSED, Bus B - PASSED)
      5.2.2.1 Optional Mode Commands - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.2.1.1 Dynamic Bus Control - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.2.1.2 Synchronize - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.2.1.2.1 Synchronize (without Data Word) - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.2.1.2.2 Synchronize (with Data Word) - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.2.1.3 Initiate Self-Test - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.2.1.4 Transmit BIT Word - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.2.1.5 Selective Transmitter Shutdown and Override - Not Tested (Bus A - Not Tested, Bus B - Not Tested)
        5.2.2.1.6 Terminal Flag Bit Inhibit and Override - Not Tested (Bus A - Not Tested, Bus B - Not Tested)
        5.2.2.1.7 Transmit Vector Word - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.2.1.8 Transmit Last Command - PASSED (Bus A - PASSED, Bus B - PASSED)

      5.2.2.2 Status Word Bits - Not Tested (Bus A - Not Tested, Bus B - Not Tested)
        5.2.2.2.1 Service Request - Not Tested (Bus A - Not Tested, Bus B - Not Tested)
        5.2.2.2.2 Broadcast Command Received - Not Tested (Bus A - Not Tested, Bus B - Not Tested)
        5.2.2.2.3 Busy - Not Tested (Bus A - Not Tested, Bus B - Not Tested)
        5.2.2.2.4 Subsystem Flag - Not Tested (Bus A - Not Tested, Bus B - Not Tested)
        5.2.2.2.5 Terminal Flag - Not Tested (Bus A - Not Tested, Bus B - Not Tested)

      5.2.2.3 Illegal Command - Not Tested (Bus A - Not Tested, Bus B - Not Tested)

      5.2.2.4 Broadcast Mode Commands - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.2.4.1 Broadcast Synchronize (without Data Word) - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.2.4.2 Broadcast Synchronize (with Data Word) - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.2.4.3 Broadcast Initiate Self-Test - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.2.4.4 Broadcast Transmitter Shutdown and Override - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.2.4.5 Broadcast Selective Transmitter Shutdown and Override - Not Tested (Bus A - Not Tested, Bus B - Not Tested)
        5.2.2.4.6 Broadcast Terminal Flag Inhibit and Override - Not Tested (Bus A - Not Tested, Bus B - Not Tested)
        5.2.2.4.7 Broadcast Reset Remote Terminal - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.2.4.8 Broadcast Dynamic Bus Control - PASSED (Bus A - PASSED, Bus B - PASSED)

      5.2.2.5 Error Injection - Broadcast Messages - PASSED (Bus A - PASSED, Bus B - PASSED)
        5.2.2.5.1 Parity: BC to RT Broadcast - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.2.5.1.1 Command Word Error - PASSED (Bus A - PASSED, Bus B - PASSED)
          5.2.2.5.1.2 Data Word Error - PASSED (Bus A - PASSED, Bus B - PASSED)

        5.2.2.5.2 Message Length: BC to RT Broadcast - PASSED (Bus A - PASSED, Bus B - PASSED)